|  |  |
| --- | --- |
| Image result for ph2 star bit | Ph2 star drill bit 50mm, magnetic |
|  |  |
| Image result for socket bit | 5/16”, 8mm ph2 socket bit, magetic  3/8”, 10mm ph2 socket nit magnet |
| note | 5/16” is 8mm (dia of socket) |
|  | 3/8” is 10mm (dia of socket) |
| Image result for carbide tipped hole saw cutter with arbor | Carbide tipped hole saw with arbor dia ranging from 20-120mm dia. For cutting on Light guage steel (1-3mm thk) |
| Image result for HSS drill bit | HSS drill bit for drilling steel (0-3mm)  M16x110mm  M12x110mm |
| Image result for sds plus concrete drill bits | Concrete drill bit SDS plus shank for drilling concrete surfaces  M12x260mm 0r 210mm  M16x210mm |
| Image result for diamond cutting disc supercut for concrete | Diamond cutting disc for concrete surfaces.  4.5” dia  9” dia |
| Related image | Cup grinding diamond disc  9” dia or 7” dia |
|  | |
| Image result for rhodius grinding disc for steel | Grinding disc for steel surfaces  4.5” dia  9” dia |